Klar, M, Jehle, M, Jähne, B, Detert, M and H., J G (2004). Analysis of subsurface gravel layer flow caused by turbulent open-channel flow using 3D PTV and pressure sensor techniques. BAW-Workshop Soil and Bed Stability - Interaction Effects between Geotechnics and Hydraulic Engineering